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SPECIFICATION:
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Suitable winding diameter range 08-2.8m
Finally completed outer diameter 150-400mm
Minimum completed inner diameter 40mm
Maximum finished height 150mm
Width of magazine 8-20mm (optional), standard: 12mm
Magazine circumference 1070mm
Maximum winding speed 230 pm
Presetable programs 50%20 groups (1000 running programs)
Overall machine weight 138kg
FEATURES:

1.Toroid Transformer Winding Machine are advanced,strongly built workhorses
capable of winding light as well as heavy wire without insulation damage.

2.The open gap gear rack and hinged gap magazine of Toroid Transformer Winding
Machine facilitate core change ,maximzing output.

3.Easily exchangeable magazines secure maximum flexbility.

4.Extremely powerful,maintenance free AC motors for main drive and core rotation.
5.High technical winding shuttle for winding by highest efficiency.

6.Toroid Transformer Winding Machine can accurately count length of loading by

limited-switch.
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7.Toroid Transformer Winding Machine can accurately count turns of winding and

taping by photo-electricity sensor.

ADVANTAGES:

1.Stable machine performance

2.Communicate parameters in a timely and thoughtful manner

3.Wide range of application, Large range of Speed adjustment, wide range of the
wire diameter, Multi-style of core, Brake tension adjustable, Good settlement for
large outer diameter, small inner diameter, heavy wire coils.

4High production efficiency, increase winding efficiency by adjustment of suitable
brake tension,

5.Each wiring part guarantee no wire damage.

6.Parts highly optimized and universal for general use, Easy maintenance

7.Complete specifications and data.

APPLICATION:
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Toroid Winding Machineis the best suited to toroidal inductor, toroidal
transformers,toroidal current transformers,toroidal coil, toroid choke coil, power

inductors,UPS inductor,converter inductor and heavy toroidal core etc.
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PRACTICAL APPLICATION :

TRAINNING CUSTOMER TO OPERATE WINDING MACHNE :

LAl service engineers with 10 years expericnce are gotten special technology train-
ing, who can deal with various breakdown problem.

2.Guide the user to use accurately and how to maintain the product.Provide free cons

ultation about production process technology of electronic products.
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3.In order to guarantee the machine used normally, we'd have training on how to ope

rate, use and maintain our product by English manual, video, guiding on line.

WhatsApp:+86 18622096679

PACKAGING:
Packaging Material: Carton/Wooden case with foam inside.
1. General package(Paper carton or plastic bag): For small euipped parts for Toroid
TransformerWindingMachine , Package it with form and pack paper to guarantee un
broken during the transport.
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2.Wooden case package: For larger scale Toroidal Winding machine
,we have special skilled

carpenter, who would make the proper wooden case with exact thickness,density,len
gth. The up arrow tmarked on the outer wooden case. Buffer material would be put i

n the wooden case to prevent crack and shock.
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FACTORY:

KIOXIALIGHT RING EUIPMENT GROUP CO. LTD.
Founded in 1993, KIOXIA LIGHT RING EUIPMENT GROUP CO.,LTD. has been a well-known manufacturing excellent
performance winding machines together with associated production and technology. KIOXIA LIGHT RING provide
highly cost effective manufacturing solutions for the production of the wound components of al types such as
transformers,chokes efc.
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